{"text_format":"2","workbook":"xlsx","n_sheets":5,"sheets":["Classification","Key information","FC -  List","FHA AIDA V4.4","DPCache_SFHA-scenario"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":1,"pivot_tables":1},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Classification","index":0,"n_rows":18,"n_cols":12,"rows_kept":18,"cut":false,"hidden":false,"merged":[[8,7,8,8]]}
[]
[]
["Idée: conserver la classification classique en associant des proabilités correspondants à la durée de vie de la flotte ou d'un drone"]
[]
["Safety",{"$nulls":6},"Pour un avion","/FH"]
["Classification","Effect on people ","Effect on goods in drone environment","Allowable qualitative probability","Allowable quantitative per flight hours","FDAL (TBC)",null,"proba d'un accident sérieux",9.9999999999999995E-7]
["CATASTROPHIQUE","Multiple serious or fatal injury ","Material destruction with major impact on safety, critical reduction of safety margins (flight in prohibited zone, uncontrolled crash)","Extremely improbable\nUnlikely at fleet level",{"$f":"I17/L17","v":5.0000000000000001E-9},"B\n\nBeware: fail safe criteria",null,"10% à cause d'une panne de systèmes",{"$f":"I6*10/100","v":9.9999999999999995E-8}]
["HAZARDOUS","Physical distress , stress or injury to a small number of people ","Material destruction.\nSignificant reduction of safety margins","Extremly remote\nFew times at fleet life level",9.9999999999999995E-8,"C",null,"On autorise 100 FC Catastrophique",{"$f":"I7/100","v":9.9999999999999986E-10}]
["MAJOR","Increase workload for operator,\nor signicative delay","Drone loss or drone Key function loss.\nReduction of safety margins\n","Remote\nUnlikely at A/C life level / several time at fleet level",1.0000000000000001E-5,"D",null,"Heures"]
["MINOR","inconvenience, small delay","Partial drone functionality loss","Probable\nOne or more times per aircraft life",1E-3,"E",null,"Nombre d'heures d'une mission",1,"valeur majorante à confirmer. 20 minute autonomie. "]
["No Safety Effects","None",null,"None",null,null,null,"Nombre d'heure de mission par an",{"$f":"10*200","v":2000},"10 missions de 1 heure par jour sur 200 jours"]
["info règlementaire et tendance de comment c'est calculé dans différents dmaine (groupes de travail)",{"$nulls":6},"Nombre de drones estimés",5000,5000,"réflexion: nombre de grosaéroport: 100\nnombre d'avion par jour de grose compagnie"]
[]
["Operability Reliability","per fligh our",{"$nulls":5},"Heure de vol 1 drone sur sa vie",{"$f":"2*I11","v":4000},"durée de vie 2 ans"]
["Mission interruption","1.e-3",{"$nulls":5},"Heure de vol flotte",{"$f":"I12*I14","v":20000000},"sur 10 ans"]
["Delay","1.e-3",{"$nulls":5},"proba/Heures","/FH"]
["No Operational effect","N/A",{"$nulls":5},"1 défaillance sur la vie de la flotte",{"$f":"1/I15","v":4.9999999999999998E-8},"proba=1 sur vie flotte","Nber FC",10]
[{"$nulls":7},"1 défaillance sur la vie du drone",{"$f":"1/I14","v":2.5000000000000001E-4}]

{"sheet":"Key information","index":1,"n_rows":33,"n_cols":14,"rows_kept":33,"cut":false,"hidden":false,"merged":[]}
["Données de la mission",null,null,"Action Christel:\nObjectif réglementaire et mise en œuvre pour notre drone.",{"$nulls":4},"Contraintes opérationnelles -> Procédures et Manual",{"$nulls":4},"Tâches de maintenance"]
["Durée de vie du drone","2 ans",null,"contenu du dossier pour avoir les autorisation de vol."]
["temps de vol","1 heures",null,"Element de référence pour positionnement des hypotèses de travail."]
["temps au sol",null,null,"par exemple définition de crash zone"]
["Décollage","1mn",null,"Scénario d'intrusion et stratégie à définir."]
["Temps croisière","<1h"]
["Atterrissage","1mn"]
["Temps de réaction pilote de drone","10s"]
[]
["List of External events"]
[null,"proba associées"]
["Obstacle entering in drone flight zone"]
["Unauthorize person  in drone flight zone"]
["A/C moving"]
["Wind Gust"]
["Rain, snow, lighntning"]
["Poor visbility condition"]
[]
[]
["List of External Function",null,null,"Contrainte de certification"]
["Data Base",null,null,"Le mode manuel est un mode de backup du mode auto"]
["Positionning signal loss"]
["Positionning signal erroneous"]
[]
["Forseen Common cause to be included in AFHA (ARP4754A)"]
[]
["Info importante:"]
["si des éléments se détachent du drones ils peuvent aussi avoir des effets critiques. Question: dans quelle analyse safety va-t-on regarder ça?  Rajouter FC, mais non reliées à une fonction"]
[]
["Hypothesis that have an impact on FC list"]
["Hyp. 1 : the drone is operated on the airport perimeter, inside an authorized flight zone around the inspected aircraft, in which the ATC ensure the absence of any other flying object (aircraft or drone)."]
["Hyp. 2 : the drone operator always have direct line of sight on the drone"]
["Hyp. 3 : normal inspection operations are always conducted in Flight Plan auto mode. The manual mode is a back-up mode, when the automatic control is not possible"]

{"sheet":"FC -  List","index":2,"n_rows":100,"n_cols":7,"rows_kept":100,"cut":false,"hidden":false,"merged":[]}
["List of Failure Conditions","FC title","S/R repercussion\nImmediate effect of failure on Drone, operator, people around","Colonne D","Colonne E","Colonne F","(vide)"]
["FC01 (CAT)","Uncontrolled drone (drone fly away) in an unauthorized area","Loss of drone uncontrolled in authorized area. Potentially crash on inspected aircraft.","FC01 (CAT)"]
[null,null,"Partial loss of thrust and loss of manual mode",null,"ok"]
[null,null,"Erroneous thrust",null,null,"Fm 1.1.2"]
["FC02 (HAZ)","Uncontrolled drone in an authorized area","Loss of drone uncontrolled in authorized area. Potentially crash on inspected aircraft.",null,null,"Fm 1.1.4"]
[null,null,"Partial loss of thrust (partially controlled by manual piloting)",null,null,"Fm 1.1.6"]
[null,null,"Total loss of thrust",null,null,"Fm 1.1.7"]
["FC03 (MAJ)","Loss of drone capability leading to mission abortion","Loss of automatic drone control",null,null,"Fm 2.1.4"]
[null,null,"Pilot is required to land the drone",null,null,"Fm 2.2.2"]
[{"$nulls":5},"Fm 2.3.3"]
["FC04 (MAJ)","Loss of drone protection","Reduction of safety margins",null,null,"Fm 2.3.4"]
[{"$nulls":5},"Fm 2.4.3"]
[{"$nulls":5},"Fm 2.4.4"]
["FC05 (Min)","Degradation of drone control",null,null,null,"Fm 2.5.3"]
["FC06 (Min)","Incapacity",null,null,null,"Fm 2.5.4"]
[{"$nulls":5},"Fm 3.1.3"]
[{"$nulls":5},"Fm 3.1.4"]
[{"$nulls":5},"Fm 3.2.3"]
[{"$nulls":5},"Fm 3.2.4"]
[{"$nulls":5},"Fm 3.3.4"]
[{"$nulls":5},"Fm 3.4.4"]
[{"$nulls":5},"Fm 4.1.3"]
[{"$nulls":5},"Fm 4.2.4"]
[{"$nulls":4},"(vide)"]
[{"$nulls":5},"Fm 6.1.4"]
[{"$nulls":5},"Fm 7.4.3"]
[null,null,null,"FC02 (HAZ)"]
[{"$nulls":4},"ok"]
[{"$nulls":5},"Fm 1.1.1"]
[{"$nulls":5},"Fm 1.1.3"]
[{"$nulls":5},"Fm 1.1.8"]
[{"$nulls":5},"Fm 2.1.3"]
[{"$nulls":5},"Fm 2.2.1"]
[{"$nulls":5},"Fm 2.3.1"]
[{"$nulls":5},"Fm 2.3.2"]
[{"$nulls":5},"Fm 2.4.1"]
[{"$nulls":5},"Fm 2.4.2"]
[{"$nulls":5},"Fm 2.5.1"]
[{"$nulls":5},"Fm 2.5.2"]
[{"$nulls":5},"Fm 3.1.1"]
[{"$nulls":5},"Fm 3.1.2"]
[{"$nulls":5},"Fm 3.2.1"]
[{"$nulls":5},"Fm 3.2.2"]
[{"$nulls":5},"Fm 3.3.2"]
[{"$nulls":5},"Fm 3.4.2"]
[{"$nulls":5},"Fm 4.2.2"]
[{"$nulls":5},"Fm.1.1.5"]
[{"$nulls":4},"(vide)"]
[{"$nulls":5},"Fm 7.1.1"]
[{"$nulls":5},"Fm 7.1.2"]
[{"$nulls":5},"Fm 7.2.1"]
[{"$nulls":5},"Fm 7.2.2"]
[{"$nulls":5},"Fm 7.3.1"]
[{"$nulls":5},"Fm 7.3.2"]
[{"$nulls":5},"Fm 7.3.3"]
[{"$nulls":5},"Fm 7.3.4"]
[{"$nulls":5},"Fm 7.3.5"]
[{"$nulls":5},"Fm 7.3.6"]
[{"$nulls":5},"Fm 7.4.2"]
[null,null,null,"FC03 (MAJ)"]
[{"$nulls":4},"ok"]
[{"$nulls":5},"Fm 2.1.1"]
[{"$nulls":5},"Fm 2.1.2"]
[{"$nulls":5},"Fm 3.3.1"]
[{"$nulls":5},"Fm 3.3.3"]
[{"$nulls":5},"Fm 3.4.1"]
[{"$nulls":5},"Fm 3.4.3"]
[{"$nulls":5},"Fm 4.1.2"]
[{"$nulls":5},"Fm 4.2.1"]
[{"$nulls":5},"Fm 4.2.3"]
[{"$nulls":5},"Fm 4.3.1"]
[{"$nulls":5},"Fm 4.3.2"]
[{"$nulls":5},"Fm 4.3.3"]
[{"$nulls":5},"Fm 4.3.4"]
[{"$nulls":5},"Fm 4.3.5"]
[{"$nulls":4},"(vide)"]
[{"$nulls":5},"Fm 4.4.1"]
[{"$nulls":5},"Fm 4.4.2"]
[{"$nulls":5},"Fm 6.1.3"]
[{"$nulls":5},"Fm 6.4.2"]
[{"$nulls":5},"Fm 6.4.3"]
[{"$nulls":5},"Fm 6.4.4"]
[null,null,null,"FC04 (Min)"]
[{"$nulls":4},"ok"]
[{"$nulls":5},"Fm 4.1.1"]
[{"$nulls":4},"(vide)"]
[{"$nulls":5},"Fm 3.4.5"]
[{"$nulls":5},"Fm 3.4.6"]
[{"$nulls":5},"Fm 4.4.3"]
[{"$nulls":5},"Fm 4.4.5"]
[{"$nulls":5},"Fm 5.1"]
[{"$nulls":5},"Fm 6.1.1"]
[{"$nulls":5},"Fm 6.2.1"]
[{"$nulls":5},"Fm 6.3.1"]
[{"$nulls":5},"Fm 6.4.1"]
[{"$nulls":5},"Fm 7.4.1"]
[null,null,null,"(vide)"]
[{"$nulls":4},"(vide)"]
[{"$nulls":5},"(vide)"]
[null,null,null,"Total Résultat"]

{"sheet":"FHA AIDA V4.4","index":3,"n_rows":27,"n_cols":11,"rows_kept":27,"cut":false,"hidden":false,"merged":[[14,0,17,0],[14,1,17,1],[19,0,22,0],[19,1,22,1],[23,0,25,0],[23,1,25,1],[2,0,3,0],[2,1,3,1],[4,0,8,0],[4,1,8,1],[9,0,13,0],[9,1,13,1]]}
[]
["Function ID","Function name","Function failure ID","Functions failures","S/R repercussion\nImmediate effect of failure on Drone, operator, people around","Detection means\nwarnings/hidden?","High level effect","Failure condition","Classification\noperability/\nreliability","parameters (procedure to detect failure, maintenance interval","Recommandation"]
["SF1","Control drone propulsion","Fm1.1","Loss of thrust","Complete loss of drone thrust. Loss of drone uncontrolled in authorized area. Potentially crash on inspected aircraft.","Detected visually by the pilot","Crash in authorized area","FC02 : Uncontrolled drone in an authorized area","HAZ"]
[null,null,"Fm1.2","Erroneous thrust","Erroneous drone control. Potentially flight in unauthorized zone leading at worst to fatalities.","Detected by the Monitoring function","Potentially flight in unauthorized zone leading at worst to fatalities.","FC01 : Uncontrolled drone (drone fly away) in an unauthorized area","CAT"]
["SF2","Control drone attitude and position","Fm2.1","Erroneous or loss of drone attitude and position control","Control loss is detected by the monitoring function. Motors are depowered. Loss of drone uncontrolled in authorized area. Potentially crash on inspected aircraft.","Detected by the monitoring function","Crash in authorized area","FC02 : Uncontrolled drone in an authorized area","HAZ"]
[null,null,"Fm2.2","Erroneous or loss of drone attitude and position control combined with loss of protection function","Control loss, not detected by the monitoring function. Potentially flight in unauthorized zone leading at worst to fatalities.","Detected visually by the pilot","Potentially flight in unauthorized zone leading at worst to fatalities.","FC01 : Uncontrolled drone (drone fly away) in an unauthorized area","CAT"]
[null,null,"Fm2.3","Erroneous or loss of drone attitude and position control, combined with incapacity to control the drone in manual mode","Drone operator cannot control the drone manual mode. In worst case, erroneous position control leads the drone out of the authorized area.","Detected visually by the pilot","Potentially flight in unauthorized zone leading at worst to fatalities.","FC01 : Uncontrolled drone (drone fly away) in an unauthorized area","CAT"]
[null,null,"Fm2.4","Partial erroneous or loss of drone attitude and position control","No effect in Manual Mode. In auto mode operator switches to Manual mode, increased workload and end of mission.","Detected visually by the pilot","Mission abortion","FC03 : Loss of drone capability leading to mission abortion","MAJ"]
[null,null,"Fm2.5","Partial erroneous or loss of drone attitude and position control combined with incapacity to control the drone in manual mode","Loss of drone uncontrolled in authorized area. Operator cannot control the drone in manual mode.\nThe drone stays more or less in the same position until the battery runs out of power.","Detected visually by the pilot","Loss of drone uncontrolled in authorized area. Potentially crash on inspected aircraft.\n","FC02 : Uncontrolled drone in an authorized area","HAZ"]
["SF3","Compute drone position and speed","Fm3.1","Erroneous or loss of drone position and speed. ","Drone control loss, detected by the monitoring function. Motors are depowered. Loss of drone uncontrolled in authorized area. Potentially crash on inspected aircraft.","Detected by the monitoring function","Crash in authorized area","FC02 : Uncontrolled drone in an authorized area","HAZ"]
[null,null,"Fm3.2","Erroneous or loss of drone position and speed combined with loss of protection function","Drone control loss, not detected by the monitoring function. Potentially flight in unauthorized zone leading at worst to fatalities.","Detected visually by the pilot","Potentially flight in unauthorized zone leading at worst to fatalities.","FC01 : Uncontrolled drone (drone fly away) in an unauthorized area","CAT"]
[null,null,"Fm3.3","Erroneous or loss or drone position and speed combined with incapacity to control the drone in manual mode","Drone operator cannot control the drone manual mode. In worst case, erroneous position control leads the drone out of the authorized area.","Detected visually by the pilot","Potentially flight in unauthorized zone leading at worst to fatalities.","FC01 : Uncontrolled drone (drone fly away) in an unauthorized area","CAT"]
[null,null,"Fm3.4","Partial erroneous or loss of drone position and speed","No effect in Manual Mode. In auto mode operator switches to Manual mode, increased workload and end of mission.","Detected visually by the pilot","Mission abortion","FC03 : Loss of drone capability leading to mission abortion","MAJ"]
[null,null,"Fm3.5","Partial erroneous or loss of drone position and speed combined with incapacity to control the drone in manual mode","Loss of drone uncontrolled in authorized area. Operator cannot control the drone in manual mode.\nThe drone stays more or less in the same position until the battery runs out of power.","Detected visually by the pilot","Loss of drone uncontrolled in authorized area. Potentially crash on inspected aircraft.\n","FC02 : Uncontrolled drone in an authorized area","HAZ"]
["SF4","Control drone navigation","Fm4.1","Erroneous or loss of drone navigation control in auto mode","The operator detects it and switches to Manual mode, increased workload and end of mission.","Detected visually by the pilot","Mission abortion","FC03 : Loss of drone capability leading to mission abortion","MAJ"]
[null,null,"Fm4.2","Loss of drone navigation control in manual mode","Incapacity to control the drone in manual mode. No effect without additional failure. ","None","Reduction of safety margin","FC04 : loss of drone monitoring","MAJ"]
[null,null,"Fm4.3","Erroneous drone navigation control in manual mode after loss of auto mode","The operator detects but cannot control the drone in manual mode. In worst case, erroneous position control leads the drone out of the authorized area.","Detected visually by the pilot","Potentially flight in unauthorized zone leading at worst to fatalities.","FC01 : Uncontrolled drone (drone fly away) in an unauthorized area","CAT"]
[null,null,"Fm4.4","Erroneous drone navigation control in manual mode","Worst case : inadvertent manual mode selection and erroneous control leading the drone out of the authorized area.","Detected visually by the pilot","Potentially flight in unauthorized zone leading at worst to fatalities.","FC01 : Uncontrolled drone (drone fly away) in an unauthorized area","CAT"]
["SF5","Make and record video","Fm5.1","Incapacity to record video","Aircraft inspection fails. ","Detected by the pilot at the end of the mission",null,"No safety effect","NSE",null,"Design objective : 10-3"]
["SF6","Manage mission","Fm6.1","Erroneous or loss of mission management leading to incapacity to control the drone in auto mode","If flight plan invalid before flight : automatic inspection not possible\nIf flight plan invalid during flight (while in auto inspection mode)  : interruption of the automatic inspection sequence, the pilot has to switch to manual control (position stabilisation) and abort the mission","Detected visually by the pilot","Mission abortion","FC03 : Loss of drone capability leading to mission abortion","MAJ"]
[null,null,"Fm6.3","Erroneous or loss of mission management leading to erroneous or loss of flight plan combined with incapacity to control the drone in manual mode","Operator will detect visually the erroneous behavior and will select the manual mode without regaining control. Potentially flight in non authorized zone leading at worst to fatalities.","Detected visually by the pilot","Potentially flight in unauthorized zone leading at worst to fatalities.","FC01 : Uncontrolled drone (drone fly away) in an unauthorized area","CAT"]
[null,null,"Fm6.4","Loss of mission management leading to loss of inspection results","Aircraft inspection fails, detected by the operator.","Detected by the pilot at the end of the mission",null,"No safety effect","NSE"]
[null,null,"Fm6.5","Erroneous mission management leading to erroneous results analysis","Aircraft inspection fails, not detected by the operator. Worst case : aircraft defaults not warned to flight crew","None","Not covered in this analysis","Not covered in this analysis","Not covered in this analysis"]
["SF7","Monitor drone control","Fm7.1","Loss of monitoring capability","Incapacity to detect and thus to accomodate a control failure. No consequences without an additional failure","Hidden","Incapacity to accomodate a control failure --> major loss of monitoring","FC04 : loss of drone monitoring","MAJ"]
[null,null,"Fm7.2","Erroneous monitoring leading to complete loss of thrust","Total loss of thrust. The drone crashes but stay inside the authorized area","Detected visually by the pilot","Crash in authorized area","FC02 : Uncontrolled drone in an authorized area","HAZ"]
[null,null,"Fm7.3","Erroenous monitoring leading to erroneous thrust","Erroneous drone control. Potentially flight in unauthorized zone leading at worst to fatalities.","Detected visually by the pilot","Potentially flight in unauthorized zone leading at worst to fatalities.","FC01 : Uncontrolled drone (drone fly away) in an unauthorized area","CAT"]
["SF8","Provide direct remote identification information","Fm8.1","Erroneous or loss of direct remote identification information","Direct remote identification information are not broadcasted to surrounding systems","Hidden","ATC and airport authorities are not informed of drone operations.","No safety effect","NSE"]

{"sheet":"DPCache_SFHA-scenario","index":4,"n_rows":61,"n_cols":3,"rows_kept":61,"cut":false,"hidden":true,"merged":[]}
["FC","Function failure ID","Functions failures"]
[]
["FC02 (HAZ)","Fm 1.1.1","Partial loss of  helix  Control"]
["FC01 (CAT)","Fm 1.1.2","Partial loss of  helix  Control, combined with incapacity to crash the drone"]
["FC02 (HAZ)","Fm 1.1.3","Total loss of helixes control"]
["FC01 (CAT)","Fm 1.1.4","Partial loss of  helix  Control, combined with loss of quick control recovery "]
["FC01 (CAT)","Fm 1.1.5","Erroneous Control of one helix"]
["FC02 (HAZ)","Fm 1.1.6","Symetrical loss of two helixes "]
["FC01 (CAT)","Fm 1.1.7","Symetrical loss of two helixes, combined with incapacity to crash the drone"]
["FC02 (HAZ)","Fm 1.1.8","Assymetrical loss of two helixes"]
["FC01 (CAT)","Fm 1.1.9","Assymetrical loss of two helixes, combined with incapacity to crash the drone"]
[]
["FC04 (Min)","Fm 2.1.1","Loss of control of drone position in auto mode"]
["FC04 (Min)","Fm 2.1.2","Erroneous control of drone position in auto mode"]
["FC02 (HAZ)","Fm 2.1.3","Loss of control of drone position in manual mode"]
["FC01 (CAT)","Fm 2.1.4","Erroneous control of drone position in manual mode"]
["FC02 (HAZ)","Fm 2.1.5","Loss of drone position in both auto and manual mode"]
["FC01 (CAT)","Fm 2.1.6","Erroneous drone position in both auto and manual mode"]
["FC02 (HAZ)","Fm 2.2.1","Loss of acquisition of pilot order in manual mode"]
["FC01 (CAT)","Fm 2.2.2","Erroneous acquisition of pilot order in manual mode"]
["FC02 (HAZ)","Fm 2.3.1","Loss of attitude control "]
["FC01 (CAT)","Fm 2.3.2","Erroneous control of attitude"]
["FC02 (HAZ)","Fm 2.4.1","Loss of altitude control "]
["FC01 (CAT)","Fm 2.4.2","Erroneous control of altitude"]
["FC03 (MAJ)","Fm 2.5.1","Loss of thrust control"]
["FC01 (CAT)","Fm 2.5.2","Erroneous thrust control"]
[]
["FC02 (HAZ)","Fm 3.1.1","Loss of drone attitude computation"]
["FC01 (CAT)","Fm 3.1.2","Erroneous attitude computation"]
["FC02 (HAZ)","Fm 3.2.1","Loss of drone altitude computation"]
["FC01 (CAT)","Fm 3.2.2","Erroneous altitude computation"]
["FC04 (Min)","Fm 3.3.1","Loss of drone speed computation"]
["FC02 (HAZ)","Fm 3.3.2","Loss of drone speed computation, combined with loss of manual mode"]
["FC04 (Min)","Fm 3.3.3","Erroneous speed computation"]
["FC01 (CAT)","Fm 3.3.4","Erroneous speed computation, combined with loss of manual mode"]
["FC04 (Min)","Fm 3.4.1","Loss of drone position computation"]
["FC02 (HAZ)","Fm 3.4.2","Loss of drone position computation, combined with loss of manual mode"]
["FC04 (Min)","Fm 3.4.3","Erroneous position computation"]
["FC01 (CAT)","Fm 3.4.4","Erroneous position computation, combined with loss of manual mode"]
["FC04 (Min)","Fm 3.4.5","Loss of time computation"]
[null,null,"Loss of time computation, combined with loss of manual mode"]
["FC04 (Min)","Fm 3.4.6","Erroneous time computation"]
[null,null,"Erroneous time computation, combined with loss of manual mode"]
[]
["FC03 (MAJ)","Fm 4.1.1","Loss of acquisition or flight plan storage"]
["FC03 (MAJ)","Fm 4.1.2","Erroneous  acquisition or flight plan storage"]
["FC01 (CAT)","Fm 4.1.3","Erroneous acquisition of flight plan, combined with loss of manual mode"]
["FC03 (MAJ)","Fm 4.2.1","Loss of the ability to run planned flight plan"]
["FC01 (CAT)","Fm 4.2.2","Loss of the ability to run planned flight plan, combined with loss of manual mode"]
["FC03 (MAJ)","Fm 4.2.3","Erroneous flight plan run "]
["FC01 (CAT)","Fm 4.2.4","Erroneous flight plan run, combined with loss of manual mode"]
["FC03 (MAJ)","Fm 4.3.1","Loss of MAN or AUTO selection"]
["FC01 (CAT)","Fm 4.3.2","Erroneous AUTO mode  while in MAN mode"]
["FC03 (MAJ)","Fm 4.3.3","Erroneous MAN mode while in AUTO mode"]
["NSE"]
[]
["FC04 (Min)","Fm 6.1.1","Loss of flight plan or flight zone computation"]
["FC01 (CAT)","Fm 6.1.2","Erroneous flight plan or flight zone computation"]
["NSE"]
[]
["NSE"]