{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["ReadME","Requirements for system level"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"ReadME","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Requirements for system level","index":1,"n_rows":29,"n_cols":9,"rows_kept":29,"cut":false,"hidden":false,"merged":[[0,7,0,8],[2,0,4,0],[6,0,16,0],[17,0,22,0],[23,0,28,0],[0,3,0,4],[0,5,0,6]]}
["System","List of Failure Conditions","FC title","Requirements from FC01 (CAT) analyse",null,"Requirements from FC02 (HAZ) analyse",null,"Synthesis"]
[null,null,null,"Criticity","Failure rate objective (if more severe than required by the criticity), 1/fh","Criticity","Failure rate objective (if more severe than required by the criticity), 1/fh","Criticity","Failure rate objective (if more severe than required by the criticity), 1/fh"]
["Propulsion system","FC_prop_01","Erroneous thrust due to Propulsion system","CAT","1.10-9",null,null,"CAT","1.10-9"]
[null,"FC_prop_02","Incapacity to depower actuators due to Propulsion system","HAZ",null,null,null,"HAZ"]
[null,"FC_prop_03","Complete loss of thrust due to Propulsion system","N/A",null,"HAZ","1.10-7","HAZ","1.10-7"]
["Structure","FC_struct_01","Erroneous thrust due to Structure","CAT","1.10-9",null,null,"CAT","1.10-9"]
["Flight control system","FC_control_01","Erroneous desactivation of at most 3 engines","CAT","1.10-9",null,null,"CAT","1.10-9"]
[null,"FC_control_02","Erroneous attitude/altitude control","HAZ",null,null,null,"HAZ"]
[null,"FC_control_03","Erroneous attitude/altitude control combined with incapacity to depower actuators due to Flight control system","CAT","1.10-9",null,null,"CAT","1.10-9"]
[null,"FC_control_04","Erroneous position control due to Flight control system","HAZ",null,null,null,"HAZ"]
[null,"FC_control_05","Erroneous control mode selection (\"stuck auto\")","HAZ",null,"MAJ",null,"HAZ"]
[null,"FC_control_06","Erroneous position control combined with erroneous control mode selection (\"stuck auto\")","CAT","1.10-9",null,null,"CAT","1.10-9"]
[null,"FC_control_07","Erroneous control mode selection (\"stuck man\")","HAZ",null,"MAJ",null,"HAZ"]
[null,"FC_control_08","Complete loss of thrust due to Flight Control system","N/A",null,"HAZ","1.10-7","HAZ","1.10-7"]
[null,"FC_control_09","Loss of position control in AUTO mode due to Flight Control System","N/A",null,"MAJ",null,"MAJ"]
[null,"FC_control_10","Loss of position control in AUTO mode combined with erroneous control mode selection (\"stuck auto\")","N/A",null,"HAZ","1.10-7","HAZ","1.10-7"]
[null,"FC_control_11","Incapacity to depower actuators due to Flight Control system","HAZ",null,null,null,"HAZ"]
["Control desk","FC_desk_01","Erroneous flight plan computation","HAZ",null,null,null,"HAZ"]
[null,"FC_desk_02","Erroneous pilot consigns acquisition on control desk","HAZ",null,null,null,"HAZ"]
[null,"FC_desk_03","Erroneous pilot control mode acquisition","HAZ",null,"MAJ",null,"HAZ"]
[null,"FC_desk_04","Erroneous or loss of drone follow-up data display","HAZ",null,"MAJ",null,"HAZ"]
[null,"FC_desk_05","Loss of Flight plan and Flight zone computation","N/A",null,"MAJ",null,"MAJ"]
[null,"FC_desk_06","Loss of pilot consigns acquisition on control desk","N/A",null,"MAJ",null,"MAJ"]
["Remote control","FC_remote_01","Erroneous pilot consigns acquisition on remote control (other than manual override)","HAZ",null,null,null,"HAZ"]
[null,"FC_remote_02","Loss of manual override acquisition","HAZ",null,"MAJ",null,"HAZ"]
[null,"FC_remote_03","Erroneous pilot consigns acquisition on remote control combined with erroneous manual override acquisition","CAT","1.10-9",null,null,"CAT","1.10-9"]
[null,"FC_remote_04","Loss of pilot consigns acquisition on remote control (other than manual override)","N/A",null,"MAJ",null,"MAJ"]
[null,"FC_remote_05","Loss of pilot consigns acquisition combined with erroneous manual override acquisition on remote control","N/A",null,"HAZ","1.10-7","HAZ","1.10-7"]
[null,"FC_remote_06","Erroneous manual override acquisition on remote control","HAZ",null,"MAJ",null,"HAZ"]