{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Feuil1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Feuil1","index":0,"n_rows":12,"n_cols":8,"rows_kept":12,"cut":false,"hidden":false,"merged":[[11,2,11,3],[6,2,6,4],[6,5,6,6],[0,1,0,4],[0,5,0,7],[7,2,7,3],[8,2,8,3],[9,2,9,3],[10,2,10,3]]}
[null,"Safety objectives",null,null,null,"Compliance"]
[null,"List of Failure Conditions","FC title","Criticity","Failure rate objective","Achieved failure rate","\"No single failure\" criteria","Compliance"]
[null,"FC_prop_01","Erroneous thrust due to Propulsion system","CAT","1.10^-9","4,35.10^-6","Not respected","NO"]
[null,"FC_prop_02","Incapacity to depower actuators due to Propulsion system","HAZ","1.10^-6","2,6.10^-7","N/A","YES"]
[null,"FC_prop_03","Complete loss of thrust due to Propulsion system","HAZ","1.10^-7","2,3.10^-7","N/A","NO"]
[]
[null,null,"DAL requirements",null,null,"Compliance"]
[null,null,"Function",null,"Allocated FDAL","Achieved FDAL","Compliance"]
[null,null,"Control propeller 1",null,"A","A","YES"]
[null,null,"Control propeller 2",null,"A","A","YES"]
[null,null,"Control propeller 3",null,"A","A","YES"]
[null,null,"Control propeller 4",null,"A","A","YES"]